    // FIXME: is it a typo here or in IRIS itself: Perspective or Prespective ?
    "Prespective from geosync","Equidistant cylindrical","Gnomonic",
   /* 160 */ {"Bas_St_Wol", "Untergrenze strat. Bew|lkung", "hft", UC_NONE},
   /* 161 */ {"Bas_St_Wol", "Untergrenze strat. Bew|lkung", "hPa", UC_NONE},
   /* 164 */ {"Top_St_Wol", "Obergrenze strat. Bew|lkung", "hft", UC_NONE},
   /* 165 */ {"Top_St_Wol", "Obergrenze strat. Bew|lkung", "hPa", UC_NONE},
              "Icing Regime 1.Guess(1=gen,2=conv,3=strat,4=freez)", "1",
              "Icing Regime(1=general,2=convect,3=strat,4=freez)", "1",
 * The generated swig_type_info structures are assigned staticly to an initial 
 * The generated swig_type_info structures are assigned staticly to an initial
            YUR = 0.0;
            YUR = oES.YUR;
        double YUR;
    l_segment->YUR = seg_data.GetDouble(nPos+215, 22);
    seg_data.Put(psOrbit->YUR,nPos+215,22,"%22.14f");
/* Putting statics in headers is trouble. */
  /* When multiple interpeters are used, a module could have already been initialized in
    const char* pszNAM = record->GetStringSubfield("DSI", 0, "NAM", 0);
                    const char* pszNAM = record->GetStringSubfield("FDR", iFDRFieldInstance++, "NAM", 0);
                                                "PRT!NAM",
    sizeOfFields[nFields] += WriteSubFieldStr(fd, osBaseFileName, 8); /* NAM */
    sizeOfFields[nFields] += WriteSubFieldStr(fd, osNAM.c_str(), 8); /* NAM */
                                                  "NAM!STR!PRT!SWO!SWA!NEO!NEA",
        sizeOfFields[nFields] += WriteSubFieldStr(fd, osBaseFileName, 8); // NAM
      {136, "Socialist Republic of Viet Nam"},
		double	eps[NANGLES], ua, va, ang, epsa;
				ang = uv2ang(ua, va);
				i = (int) ang;
				epsa = fabs(ang - (i+.5));
                "     UN=Metres,SD=HHWLT,DX=2.500000,DY=2.500000\n");
        pszUnitsPer = CPLGetXMLValue( psSrcXML, "metresPerUnit", NULL );
    {"kilometre",    /* 15 */ 12,  13,  1000.0},
                    oSRS.SetLinearUnits( "kilometre", 1000.0 );
{ "kilometre", SRS_UL_KILOMETER_CONV, "km" }, // Leave as 'kilometre' instead of SRS_UL_KILOMETER due to historical usage
            passport.stMapDescription.eUnitInPlan = SXF_COORD_MU_CENTIMETRE;
            passport.stMapDescription.eUnitInPlan = SXF_COORD_MU_MILLIMETRE;
    SXF_COORD_MU_CENTIMETRE,
    SXF_COORD_MU_MILLIMETRE,
      addSimpleType(&oTypes, "GVAKT_PROS", "geoVernAktivProsess", OFTString);
      addSimpleType(&oTypes, "GVVKT_PROS", "geoVernViktigProsess", OFTString);
      addSimpleType(&oTypes, "PROSESS_HISTORIE", "prosesshistorie", OFTString);
            ih.Put( "<unintialized>", 64, 64 );  // TODO: Spelling?
      {7, 110, "NAM Model - 15km version"},
      {7, 111, "NAM model, generic resolution"},
      {7, 115, "Downscaled GFS from NAM eXtension"},
      {7, 130, "Merge of fields from the RUC, NAM, and Spectral Model"},
   /* 0 */ {"ACCES", "Air concentration of Caesium 137", "Bq/(m^3)", UC_NONE},
        : CPLGetXMLValue( psSrcXML, "metresPerUnit", NULL );
{ "kilometre", SRS_UL_KILOMETER_CONV, "km" },
    { CADObject::DIMENSION_ANG_3PT,    "DIMENSION ANG 3PT" },
    {"SCALING_FACTOR_ATM_PRES",                           16, EDT_Float32,     1},
    {"SCALING_FACTOR_SURF_PRES",                         104, EDT_Float32,     1},
    {"OFFSET_SURF_PRES",                                 208, EDT_Float32,     1},
  /* now prec is nonzero iff there are any 16-bit quant tables. */
   * a box is splittable iff norm > 0.
  boolean saw_JFIF_marker;	/* TRUE iff a JFIF APP0 marker was found */
  boolean saw_Adobe_marker;	/* TRUE iff an Adobe APP14 marker was found */
        // We will update the object count iff we are writing beyond the end.
   /* 1 */ {"PRES", "Pressure", "Pa", UC_NONE},
   /* 1 */ {"PRES", "Pressure", "hPa", UC_NONE},
   /* 0 */ {"PRES", "Pressure", "Pa", UC_NONE},
 * copied iff they didn't exist before.  ColorTransIn2 maps the old
      nearzero iff determinant < qh NEARzero[dim-1]
      facet->visitid= 0 iff vertex-at-infinity (i.e., unbounded)
    sets same iff vertices have the same orientation
      nearzero iff diagonal[k] < qh NEARzero[k]
ogr2ogr --config OGR_STROKE_CURVE TRUE -SQL 'SELECT Rechtsstatus,publiziertAb,MetadatenGeobasisdaten,Eigentumsbeschraenkung,ZustaendigeStelle,Flaeche FROM "OeREBKRM09trsfr.Transferstruktur.Geometrie"' shpdir ch.bazl.sicherheitszonenplan.oereb_20131118.xtf,OeREBKRM09vs.imd OeREBKRM09trsfr.Transferstruktur.Geometrie
   /* 130 */ {"MSLET", "Mean Sea Level Pressure (NAM Model Reduction)", "Pa", UC_NONE},
      addSimpleType(&oTypes, "INST_EFFEKT", "installertEffekt", OFTInteger);
