D2I_ASN1_OCTET_STRING(3)

NAME
d2i_ASN1_OCTET_STRING, i2d_ASN1_OCTET_STRING, d2i_ASN1_BIT_STRING, i2d_ASN1_BIT_STRING, d2i_ASN1_INTEGER, i2d_ASN1_INTEGER, d2i_ASN1_UINTEGER, d2i_ASN1_ENUMERATED, i2d_ASN1_ENUMERATED, d2i_ASN1_UTF8STRING, i2d_ASN1_UTF8STRING, d2i_ASN1_IA5STRING, i2d_ASN1_IA5STRING, d2i_ASN1_UNIVERSALSTRING, i2d_ASN1_UNIVERSALSTRING, d2i_ASN1_BMPSTRING, i2d_ASN1_BMPSTRING, d2i_ASN1_GENERALSTRING, i2d_ASN1_GENERALSTRING, d2i_ASN1_T61STRING, i2d_ASN1_T61STRING, d2i_ASN1_VISIBLESTRING, i2d_ASN1_VISIBLESTRING, d2i_ASN1_PRINTABLESTRING, i2d_ASN1_PRINTABLESTRING, d2i_ASN1_PRINTABLE, i2d_ASN1_PRINTABLE, d2i_DIRECTORYSTRING, i2d_DIRECTORYSTRING, d2i_DISPLAYTEXT, i2d_DISPLAYTEXT, d2i_ASN1_GENERALIZEDTIME, i2d_ASN1_GENERALIZEDTIME, d2i_ASN1_UTCTIME, i2d_ASN1_UTCTIME, d2i_ASN1_TIME_new, i2d_ASN1_TIME_new - decode and encode ASN1_STRING objects

SYNOPSIS
#include <openssl/asn1.h>
ASN1_OCTET_STRING *
d2i_ASN1_OCTET_STRING(ASN1_OCTET_STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_OCTET_STRING(ASN1_OCTET_STRING *val_in, unsigned char **der_out);
ASN1_BIT_STRING *
d2i_ASN1_BIT_STRING(ASN1_BIT_STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_BIT_STRING(ASN1_BIT_STRING *val_in, unsigned char **der_out);
ASN1_INTEGER *
d2i_ASN1_INTEGER(ASN1_INTEGER **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_INTEGER(ASN1_INTEGER *val_in, unsigned char **der_out);
ASN1_INTEGER *
d2i_ASN1_UINTEGER(ASN1_INTEGER **val_out, const unsigned char **der_in, long length);
ASN1_ENUMERATED *
d2i_ASN1_ENUMERATED(ASN1_ENUMERATED **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_ENUMERATED(ASN1_ENUMERATED *val_in, unsigned char **der_out);
ASN1_UTF8STRING *
d2i_ASN1_UTF8STRING(ASN1_UTF8STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_UTF8STRING(ASN1_UTF8STRING *val_in, unsigned char **der_out);
ASN1_IA5STRING *
d2i_ASN1_IA5STRING(ASN1_IA5STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_IA5STRING(ASN1_IA5STRING *val_in, unsigned char **der_out);
ASN1_UNIVERSALSTRING *
d2i_ASN1_UNIVERSALSTRING(ASN1_UNIVERSALSTRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_UNIVERSALSTRING(ASN1_UNIVERSALSTRING *val_in, unsigned char **der_out);
ASN1_BMPSTRING *
d2i_ASN1_BMPSTRING(ASN1_BMPSTRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_BMPSTRING(ASN1_BMPSTRING *val_in, unsigned char **der_out);
ASN1_GENERALSTRING *
d2i_ASN1_GENERALSTRING(ASN1_GENERALSTRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_GENERALSTRING(ASN1_GENERALSTRING *val_in, unsigned char **der_out);
ASN1_T61STRING *
d2i_ASN1_T61STRING(ASN1_T61STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_T61STRING(ASN1_T61STRING *val_in, unsigned char **der_out);
ASN1_VISIBLESTRING *
d2i_ASN1_VISIBLESTRING(ASN1_VISIBLESTRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_VISIBLESTRING(ASN1_VISIBLESTRING *val_in, unsigned char **der_out);
ASN1_PRINTABLESTRING *
d2i_ASN1_PRINTABLESTRING(ASN1_PRINTABLESTRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_PRINTABLESTRING(ASN1_PRINTABLESTRING *val_in, unsigned char **der_out);
ASN1_STRING *
d2i_ASN1_PRINTABLE(ASN1_STRING **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_PRINTABLE(ASN1_STRING *val_in, unsigned char **der_out);
ASN1_STRING *
d2i_DIRECTORYSTRING(ASN1_STRING **val_out, const unsigned char **der_in, long length);
int
i2d_DIRECTORYSTRING(ASN1_STRING *val_in, unsigned char **der_out);
ASN1_STRING *
d2i_DISPLAYTEXT(ASN1_STRING **val_out, const unsigned char **der_in, long length);
int
i2d_DISPLAYTEXT(ASN1_STRING *val_in, unsigned char **der_out);
ASN1_GENERALIZEDTIME *
d2i_ASN1_GENERALIZEDTIME(ASN1_GENERALIZEDTIME **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_GENERALIZEDTIME(ASN1_GENERALIZEDTIME *val_in, unsigned char **der_out);
ASN1_UTCTIME *
d2i_ASN1_UTCTIME(ASN1_UTCTIME **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_UTCTIME(ASN1_UTCTIME *val_in, unsigned char **der_out);
ASN1_TIME *
d2i_ASN1_TIME(ASN1_TIME **val_out, const unsigned char **der_in, long length);
int
i2d_ASN1_TIME(ASN1_TIME *val_in, unsigned char **der_out);

DESCRIPTION
These functions decode and encode various ASN.1 built-in types that can be represented by ASN1_STRING objects. For details about the semantics, examples, caveats, and bugs, see ASN1_item_d2i(3).

The format consists of one identifier octet, one or more length octets, and one or more content octets. The identifier octets and corresponding ASN.1 types are as follows:
OpenSSL type | identifier | ASN.1 type
 |
ASN1_OCTET_STRING | 0x04 | OCTET STRING
ASN1_BIT_STRING | 0x03 | BIT STRING
ASN1_INTEGER | 0x02 | INTEGER
ASN1_ENUMERATED | 0x0a | ENUMERATED
ASN1_UTF8STRING | 0x0c | UTF8String
ASN1_IA5STRING | 0x16 | IA5String
ASN1_UNIVERSALSTRING | 0x1c | UniversalString
ASN1_BMPSTRING | 0x1e | BMPString
ASN1_GENERALSTRING | 0x1b | GeneralString
ASN1_T61STRING | 0x14 | T61String
ASN1_VISIBLESTRING | 0x1a | VisibleString
ASN1_PRINTABLESTRING | 0x13 | PrintableString
ASN1_GENERALIZEDTIME | 0x18 | GeneralizedTime
ASN1_UTCTIME | 0x17 | UTCTime

d2i_DIRECTORYSTRING() and i2d_DIRECTORYSTRING() decode and encode an ASN.1 DirectoryString structure defined in RFC 5280 section 4.1.2.4 and used for ASN.1 EDIPartyName structures; see EDIPARTYNAME_new(3). When decoding, it accepts any of the types UTF8String, UniversalString, BMPString, T61String, or PrintableString. When encoding, it writes out the character string type that is actually passed in.

d2i_ASN1_PRINTABLE() and i2d_ASN1_PRINTABLE() are non-standard variants of d2i_DIRECTORYSTRING() and i2d_DIRECTORYSTRING() that also accept IA5String, NumericString, BIT STRING, and SEQUENCE ASN.1 values as well as ASN.1 values with unknown identifier octets (0x07, 0x08, 0x09, 0x0b, 0x0d, 0x0e, 0x0f, 0x1d, and 0x1f). Even though the standard requires the use of DirectoryString in the relative distinguished names described in X509_NAME_ENTRY_new(3), the library accepts this wider range of choices.

d2i_DISPLAYTEXT() and i2d_DISPLAYTEXT() decode and encode an ASN.1 DisplayText structure defined in RFC 5280 section 4.2.1.4 and used for ASN.1 UserNotice structures in certificate policies; see USERNOTICE_new(3). When decoding, it accepts any of the types UTF8String, IA5String, BMPString, or VisibleString. When encoding, it writes out the character string type that is actually passed in.

d2i_ASN1_TIME() and i2d_ASN1_TIME() decode and encode an ASN.1 Time structure defined in RFC 5280 section 4.1 and used for ASN.1 Validity structures in certificates; see X509_VAL_new(3). They are also used for certificate revocation lists; see X509_CRL_INFO_new(3). When decoding, it accepts either GeneralizedTime or UTCTime. When encoding, it writes out the time type that is actually passed in.

d2i_ASN1_UINTEGER() is similar to d2i_ASN1_INTEGER() except that it ignores the sign bit in the BER encoding and treats all integers as positive. It helps to process BER input produced by broken software that neglects adding a leading NUL content byte where required.

RETURN VALUES
The d2i_*() decoding functions return an ASN1_STRING object or NULL if an error occurs.

The i2d_*() encoding functions return the number of bytes successfully encoded or a negative value if an error occurs.

SEE ALSO
ASN1_item_d2i(3), ASN1_STRING_new(3)

STANDARDS
ITU-T Recommendation X.680, also known as ISO/IEC 8824-1: Information technology - Abstract Syntax Notation One (ASN.1): Specification of basic notation

RFC 5280: Internet X.509 Public Key Infrastructure Certificate and Certificate Revocation List (CRL) Profile