[comment {-*- tcl -*- doctools manpage}]
[vset PACKAGE_VERSION 0.5.2]
[manpage_begin nettool n [vset PACKAGE_VERSION]]
[keywords {nettool}]
[keywords {odie}]
[copyright {2015-2018 Sean Woods <yoda@etoyoc.com>}]
[moddesc   {nettool}]
[titledesc {Tools for networked applications}]
[category  System]
[require Tcl 8.5]
[require nettool [opt [vset PACKAGE_VERSION]]]
[require twapi 3.1]
[require ip 0.1]
[require platform 0.1]
[description]
[para]

The [package nettool] package consists of a Pure-tcl set of tools
to perform common network functions that would normally require
different packages or calls to exec, in a standard Tcl interface.

At present nettool has reference implementations for the following operating
systems: Windows, MacOSX, and Linux (debian).

[section Commands]
[list_begin definitions]

[call [cmd ::cat] [arg filename]]

Dump the contents of a file as a result.

[call [cmd ::nettool::allocate_port] [arg startingport]]

Attempt to allocate [arg startingport], or, if busy, advance the port
number sequentially until a free port is found, and claim that port.

This command uses a built-in database of known ports to avoid returning a
port which is in common use. (For example: http (80))

[call [cmd ::nettool::arp_table]]

Dump the contents of this computer's Address Resolution Protocol (ARP) table.
The result will be a Tcl formatted list: [arg macid] [arg ipaddrlist] ...

[call [cmd ::nettool::broadcast_list]]

Returns a list of broadcast addresses (suitable for UDP multicast)
that this computer is associated with.

[call [cmd ::nettool::claim_port] [arg port] [opt [arg protocol]]]

Mark [arg port] as busy, optionally as either [const tcp] (default) or [const udp].

[call [cmd ::nettool::cpuinfo] [arg args]]

If no arguments are given, return a key/value list describing the
CPU of the present machine. Included in the matrix is info on the number
of cores/processors that are available for parallel tasking, installed physical
RAM, and processor family.
[para]
The exact contents are platform specific.
[para]
For Linux, information is drawn from /proc/cpuinfo and /proc/meminfo.
[para]
For MacOSX, information is drawn from sysctl
[para]
For Windows, information is draw from TWAPI.
[para]
If arguments are given, the result with be a key/value list limited to the
fields requested.
[para]
Canonical fields for all platforms:
[list_begin definitions][comment {-- cpuinfofields}]
[def cpus]   Count of CPUs/cores/execution units
[def speed]  Clock speed of processor(s) in Mhz
[def memory] Installed RAM (in MB)
[def vendor] Manufacturer
[list_end]

[call [cmd ::nettool::find_port] [arg startingport]]

Return [arg startingport] if it is available, or the next free port after
[arg startingport]. Note: Unlike [cmd ::nettool::allocate_port], this
command does not claim the port.
[para]
This command uses a built-in database of known ports to avoid returning a
port which is in common use. (For example: http (80))

[call [cmd  ::nettool::hwid_list]]

Return a list of hardware specific identifiers from this computer. The source
and content will vary by platform.
[para]
For MacOSX, the motherboard serial number and macids for all network devices is returned.
[para]
For Windows, the volume serial number of C and macids for all network devices is returned.
[para]
For Linux, macids for all network devices is returned.

[call [cmd  ::nettool::ip_list]]

Return a list of IP addresses associated with this computer.

[call [cmd  ::nettool::mac_list]]

Return a list of MACIDs for the network cards attached to this machine. The MACID of the
primary network card is returned first.

[call [cmd ::nettool::network_list]]

Return a list of networks associated with this computer. Networks are formated with
[cmd ip::nativeToPrefix].

[call [cmd  ::nettool::port_busy] [arg port]]

Return true if [arg port] is claimed, false otherwise.

[call [cmd ::nettool::release_port] [arg port] [opt [arg protocol]]]

Mark [arg port] as not busy, optionally as either [const tcp] (default) or [const udp].

[call [cmd ::nettool::status]]

Return a key/value list describing the status of the computer. The output
is designed to be comparable to the output of [cmd top] for all platforms.
[para]
Common fields include:
[list_begin definitions][comment {-- statusfields}]
[def load]         Processes per processing unit
[def memory_total] Total physical RAM (MB)
[def memory_free]  Total physical RAM unused (MB)
[list_end]
 
[call [cmd ::nettool::user_data_root] [arg appname]]

Return a fully qualified path to a folder where [arg appname] should store it's data.
The path is not created, only computed, by this command.

[list_end]
[para]
[vset CATEGORY odie]
[include ../doctools2base/include/feedback.inc]
[manpage_end]
