[ Tcllib Home | Main Table Of Contents | Table Of Contents | Keyword Index | Categories | Modules | Applications ]

# controlwidget(n) 0.1 tklib "controlwidget"

## Name

controlwidget - Collection of widgets for displaying and controlling numerical values

## Table Of Contents

## Synopsis

- package require Tcl ?8.5?
- package require Tk ?8.5?
- package require snit ?2.0?
- package require controlwidget ?0.1?

- ::controlwidget::meter w args
- ::controlwidget::slider w args
- ::controlwidget::equalizerBar w args
- ::controlwidget::thermometer w args
- ::controlwidget::voltmeter w args
- ::controlwidget::tachometer w args
- ::controlwidget::rdial w args
- $widget get
- $widget set value
- ::controlwidget::led w args
- ::controlwidget::radioMatrix w args
- $led on
- $led off
- $led setstate state
- $matrix get
- $matrix set index

## Description

The controlwidget package focuses on the display and interactive control of numerical values. It mimicks several of the meters and controls found in laboratory settings but also daily life: volt meters, equalizers and tachometers to name a few. They can be seen as alternatives for the scale widget.

Note: The package has not sofar been tested extensively, and that may result in an unexpected appearance if you use sizes that are different than the defaults. Also not all options for the coloring of the various parts and fonts and so on have been tested, so that may be another source of bugs.

A last note: some parts have not been included in any option, most notably the colors of parts that require lighter and darker shades to cooperate.

## TYPES OF WIDGETS

The package distinguishes several typed of widgets:

- Vertical meters: the value of the variable is translated into a vertical position, like with the coloured bars you find on your stereo installation.

- Angle displays: the value of the variable is related to the angle of a needle, like with tachometers.

- Interactive widgets: most widgets allow you to change the value of the variable by pressing the mouse button on the needle and shifting it up and down or left and right.

- Non-interactive widgets: some widgets, like the thermometer widget, do not allow such interaction.

- Logical or choice widgets: some widgets display the values as either on/off (or true/false) or as one of a set of discrete choices.

All widgets have in common, however, that you can connect them to a variable and that changing the variable changes the display. Forthermore, all widgets have the set and get methods to interact with the value that the widget displays (whether that is stored in a global variable or not).

They also have in common that their appearance and behaviour is determined by one or more options that you can set at creation time and often later on as well. The widgets are all based on the snit package, so that the methods configure and cget are available to set and get these options.

## COMMANDS

Currently the package contains these widgets of the vertical meter type:

::controlwidget::meter w args

  Create a vertical meter consisting of an axis and a moveable arrow.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the variable to be associated with the meter

    background color

      Background color for the widget

    height pixels

      Height of the widget

    width pixels

      Width of the widget

    arrowthickness pixels

      Thickness of the displayed arrow in pixels

    arrowcolor color

      Color of the displayed arrow

    readonly boolean

      Whether the arrow can be moved interactively or not

::controlwidget::slider w args

  Create a widget containing one or more vertical sliders and an axis. You can shift the slider handles interactively via the mouse.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the (list) variable to be associated with the widget

    number integer

      Number of sliders in the widget

    background color

      Background color for the widget

    height pixels

      Height of the widget

    width pixels

      Width of the widget

    sliderthickness pixels

      Thickness of the slider handles

    sliderwidth color

      Width of the slider handles

    troughwidth color

      Width of the troughs holding the sliders

::controlwidget::equalizerBar w args

  Create a widget containing one or more vertical bars resembling those found on hifi graphical equalizers. Note that it is a read-only widget.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the (list) variable to be associated with the widget

    number integer

      Number of bars in the widget

    background color

      Background color for the widget

    height pixels

      Height of the widget

    width pixels

      Width of the widget

    barwidth pixels

      Width of the bars

    segments integer

      Number of segments the bars are divided in

    safecolor color

      Color for values lower than the warning level

    warningcolor color

      Color for values greater than the warning level

    warninglevel double

      Threshold value, determines at what level the color changes

::controlwidget::thermometer w args

  Create a thermometer widget (read-only)

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the (list) variable to be associated with the widget

    background color

      Background color for the widget

    height pixels

      Height of the widget

    width pixels

      Width of the widget

    linethickness pixels

      Thickness of the line representing the "temperature"

    linecolor color

      Color of the line

These widgets all use a vertical axis and have the following options in common for configuring the axis:

axisformat string

  Format string for formatting the numbers along the axis

axisfont string

  Name of the font to be used for the numbers

axiscolor color

  Color of the axis (including the numbers)

from color

  Lower value for the axis

to color

  Upper value for the axis

majorticks integer

  Number of major tickmarks to draw (each is labelled)

minorticks integer

  Number of minor tickmarks to draw between two major tickmarks

log boolean

  Use a logarithmic axis (true) or a linear axis (false)

The package contains the following widget based on angle displays:

::controlwidget::voltmeter w args

  Create a voltmeter-like widget.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the variable to be associated with the meter

    value value

      Value for the meter (if not associated with a variable)

    min value

      The minimum value for data in the display

    max value

      The maximum value for data in the display

    labels list

      The labels to be shown along the scale. (These are simply considered texts, so no relation with the minimum and maximum perse)

    title string

      String to be shown below the dial

    width pixels

      The width of the widget

    height pixels

      The height of the widget

    borderwidth pixels

      The width of the border surrounding the entire widget

    relief string

      The relief of the border surrounding the entire widget

    highlightthickness pixels

      The width of the border to indicate the widget has keyboard focus

    labelfont fontname

      Font of the labels to the scale

    titlefont fontname

      Font of the title below the dial

    dialcolor color

      Color of the dial holding the needle

    needlecolor color

      Color of the needle

    scalecolor color

      Color of the scale (arc and tickmarks)

    labelcolor color

      Color of the labels to the scale

    titlecolor color

      Color of the title below the dial

::controlwidget::tachometer w args

  Create a tachometer-like widget.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget. In addition to the ones given for the voltmeter widget:

    variable name

      Name of the variable to be associated with the meter

    value value

      Value for the meter (if not associated with a variable)

    dangerlevel value

      Level above which values are indicated with a different color

    dangercolor color

      Color for the values above the "danger level"

    dangerwidth pixels

      Width for the colored band indicating the "danger level"

    pincolor color

      Color for the needle and the pin

::controlwidget::rdial w args

  Create a rotating dial. You can drag the dial to change the value. With the shift button depressed the value changes slowly, with the control button depressed it changes fast.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget:

    variable name

      Name of the variable to be associated with the dial

    value value

      Value for the dial (if not associated with a variable)

    orient string

      Whether a horizontal disk/dial is required ("horizontal") or a vertical one ("vertical")

    step value

      Initial step for incrementing or decrementing the value

    slow value

      Factor on the step size for incrementing or decrementing the value slowly

    fast value

      Factor on the step size for incrementing or decrementing the value fast

    scale value

      Scale value to be applied to the actual value

    callback command

      Command to be called when the value changes

    width pixels

      The width of the widget

    height pixels

      The height of the widget

    background color

      The background color of the widget (coloring of the disk/dial)

    foreground color

      The foreground color of the widget (the marker lines)

All these widgets have the following methods:

$widget get

  Return the current value or values shown in the widget

$widget set value

  Reset the value or values shown in the widget. If the widget is associated with a variable, that variable is set as well.

  value double/list

    New value or values for the widget

Two further widgets are available, meant to display logical values:

::controlwidget::led w args

  Create a LED-like widget.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget. In addition to the ones given for the voltmeter widget:

    variable name

      Name of the variable to be associated with the LED

    size pixels

      Diameter of the LED widget

    on color

      Color to use for the "on" state

    off color

      Color to use for the "off" state

::controlwidget::radioMatrix w args

  Create a matrix of radio buttons that behaves as a single widget.

  widget w (in)

    Name of the widget to be created.

  arguments args (in)

    List of key-value pairs, controlling the appearance and behaviour of the widget. In addition to the ones given for the voltmeter widget:

    variable name

      Name of the variable to be associated with the matrix

    orient string

      The way the radio buttons are to be arranged (horizontal or vertical first)

    rows integer

      Number of rows in the matrix

    columns integer

      Number of columns in the matrix

    command list

      Command associated with the radio buttons. Invoked when the active radio button changes.

The LED widget has the following public methods:

$led on

  Set the state to "on"

$led off

  Set the state to "off"

$led setstate state

  Set the state according to the value of "state"

  state boolean (in)

    New state for the LED widget

The radioMatrix widget has two public methods:

$matrix get

  Return the index of the currently selected radio button

$matrix set index

  Select the radio button with index "index"

  index integer

    Index of the radio button to be set

## ACKNOWLEDGMENTS

The code for most of these widgets first appeared on the Wiki. In many cases, Arjen Markus merely refactored the code a bit and "snitified" some of them. The original code was developed by the following people:

- Vertical meter, LED display, radio matrix: Ron Fox

- Rotating dials: Gerhard Reithofer

- Voltmeter and tachometer: Marco Maggi

- Code for moving the needle: ?

## Keywords

controlling, displaying, numerical values, scale widget

## Copyright

Copyright © 2010 Ron Fox <rfox@...>
Copyright © 2010 Gerhard Reithofer <...@...>
Copyright © 2010 Marco Maggi <...@...>
Copyright © 2010 Arjen Markus <arjenmarkus@users.sourceforge.net>